|  |  |
| --- | --- |
|  |  |
| PRODUCT FICHE | |
| Model name | DU5446W |
| Annual Energy Consumption - AEChood | 67,8 kWh/a |
| Energy efficiency class | E |
| Fluid Dynamic Efficiency - FDE | 2,7 % |
| Fluid Dynamic Efficiency class | G |
| Light Efficiency - LEhood | 2,3 lux/W |
| Lighting Efficiency Class | G |
| Grease Filtering Efficiency - GFEhood | 74,1 % |
| Grease Filtering Efficiency class | D |
| A-waighted Sound Power Emission at minimum speed | 155 m³/h |
| Maximum Air Flow in normal use | 171 m³/h |
| Air Flow at intensive/boost setting | - |
| A-waighted Sound Power Emission at minimum speed | 60 dB(A) re 1pW |
| A-waighted Sound Power Emission at maximum speed | 59 dB(A) re 1pW |
| A-waighted Sound Power Emission at intensive or boost speed | - |
| Power consumption off mode - Po | - |
| Power consumption in standby mode - Ps | - |
| Time increase factor | 1,9 |
| Energy Efficiency Index -EEI | 108,3 |
| Measured air flow rate at best efficiency point - Qbep | 72,0 m³/h |
| Measured air pressure at best efficiency point - Pbep | 78,0 Pa |
| Maximum air flow - Qmax | 171 m³/h |
| Measured electric power input at best efficiency point - Wbep | 58,0 W |
| Nominal power of the lighting system - WL | 28,0 W |
| Average illumination of the lighting system on the cooking surface - Eaverage | 65,0 lux |